ISO-10303-21;
HEADER;
FILE_DESCRIPTION(('STEP AP214'),'1');
FILE_NAME('fter.STP','2022-01-12T13:19:53',(''),(' '),'Spatial InterOp 3D',' ','');
FILE_SCHEMA(('AUTOMOTIVE_DESIGN { 1 0 10303 214 1 1 1 1 }'));
ENDSEC;
DATA;
#2=PRODUCT_DEFINITION_CONTEXT('',#163,'design');
#3=APPLICATION_PROTOCOL_DEFINITION('INTERNATIONAL STANDARD','automotive_design',1994,#163);
#6= (GEOMETRIC_REPRESENTATION_CONTEXT(3)GLOBAL_UNCERTAINTY_ASSIGNED_CONTEXT((#170))GLOBAL_UNIT_ASSIGNED_CONTEXT((#172,#173,#174))REPRESENTATION_CONTEXT('NONE','WORKSPACE'));
#163=APPLICATION_CONTEXT(' ');
#164=PRODUCT_CATEGORY('part','NONE');
#165=PRODUCT_RELATED_PRODUCT_CATEGORY('detail',' ',(#479));
#166=PRODUCT_DEFINITION_SHAPE('NONE','NONE',#480);
#170=UNCERTAINTY_MEASURE_WITH_UNIT(LENGTH_MEASURE(1.0E-06),#172,'','');
#172= (CONVERSION_BASED_UNIT('MILLIMETRE',#484)LENGTH_UNIT()NAMED_UNIT(#487));
#173= (NAMED_UNIT(#489)PLANE_ANGLE_UNIT()SI_UNIT($,.RADIAN.));
#174= (NAMED_UNIT(#489)SOLID_ANGLE_UNIT()SI_UNIT($,.STERADIAN.));
#479=PRODUCT('XK049.A1 Heatspreader PCM-070  PL1549 mit Kühlrippen und Lüfter','','PART--DESC',(#964));
#480=PRODUCT_DEFINITION('','NONE',#965,#2);
#484=LENGTH_MEASURE_WITH_UNIT(LENGTH_MEASURE(1.0),#969);
#487=DIMENSIONAL_EXPONENTS(1.0,0.0,0.0,0.0,0.0,0.0,0.0);
#489=DIMENSIONAL_EXPONENTS(0.0,0.0,0.0,0.0,0.0,0.0,0.0);
#964=PRODUCT_CONTEXT('',#163,'mechanical');
#965=PRODUCT_DEFINITION_FORMATION_WITH_SPECIFIED_SOURCE(' ','NONE',#479,.NOT_KNOWN.);
#969= (NAMED_UNIT(#487)LENGTH_UNIT()SI_UNIT(.MILLI.,.METRE.));
ENDSEC;
END-ISO-10303-21;